Net fpga_0_clk_1_sys_clk_pin TNM_NET = sys_clk_pin;
TIMESPEC TS_sys_clk_pin = PERIOD sys_clk_pin 50000 kHz;
Net fpga_0_rst_1_sys_rst_pin TIG;

Net fpga_0_clk_1_sys_clk_pin LOC=T9;
Net fpga_0_rst_1_sys_rst_pin LOC=L14;

Net fpga_0_RX_pin LOC=T13;
Net fpga_0_TX_pin LOC=R13;

Net fpga_0_led7seg_segments_pin<0>  LOC=E14;	#segment-A
Net fpga_0_led7seg_segments_pin<1>  LOC=G13;	#segment-B
Net fpga_0_led7seg_segments_pin<2>  LOC=N15;	#segment-C
Net fpga_0_led7seg_segments_pin<3>  LOC=P15;	#segment-D
Net fpga_0_led7seg_segments_pin<4>  LOC=R16;	#segment-E
Net fpga_0_led7seg_segments_pin<5>  LOC=F13;	#segment-F
Net fpga_0_led7seg_segments_pin<6>  LOC=N16;	#segment-G
Net fpga_0_led7seg_dot_pin	         LOC=P16;	#dot
Net fpga_0_led7seg_anodes_pin<0>    LOC=D14;	#anode-0
Net fpga_0_led7seg_anodes_pin<1>    LOC=G14;	#anode-1
Net fpga_0_led7seg_anodes_pin<2>    LOC=F14;	#anode-2
Net fpga_0_led7seg_anodes_pin<3>    LOC=E13; #anode-3

Net fpga_0_led7seg_zeros_pin        LOC=K13;
Net fpga_0_led7seg_off_pin          LOC=K14;