
# ##############################################################################
# Created by Base System Builder Wizard for Xilinx EDK 13.1 Build EDK_O.40d
# Target Board:  Custom
# Family:    spartan3
# Device:    xc3s50
# Package:   pq208
# Speed Grade:  -4
# Processor number: 1
# Processor 1: microblaze_0
# System clock frequency: 66.7
# Debug Interface: On-Chip HW Debug Module
# ##############################################################################
 PARAMETER VERSION = 2.1.0


 PORT fpga_0_clk_1_sys_clk_pin = CLK_S, DIR = I, SIGIS = CLK, CLK_FREQ = 50000000
 PORT fpga_0_rst_1_sys_rst_pin = sys_rst_s, DIR = I, SIGIS = RST, RST_POLARITY = 1
 PORT fpga_0_RX_pin = rs232_RX, DIR = I
 PORT fpga_0_TX_pin = rs232_TX, DIR = O
 PORT fpga_0_led7seg_dot_pin = net_vcc, DIR = O
 PORT fpga_0_led7seg_segments_pin = led7seg_segments, DIR = O, VEC = [6:0]
 PORT fpga_0_led7seg_anodes_pin = led7seg_anodes, DIR = O, VEC = [3:0]
 PORT fpga_0_led7seg_zeros_pin = led7seg_switch_zeros, DIR = I
 PORT fpga_0_led7seg_off_pin = led7seg_switch_off, DIR = I


BEGIN xps_uartlite
 PARAMETER INSTANCE = rs232
 PARAMETER HW_VER = 1.01.a
 PARAMETER C_BAUDRATE = 115200
 PARAMETER C_USE_PARITY = 0
 PARAMETER C_BASEADDR = 0x84000000
 PARAMETER C_HIGHADDR = 0x8400ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT RX = rs232_RX
 PORT TX = rs232_TX
 PORT Interrupt = rs232_Interrupt
END

BEGIN proc_sys_reset
 PARAMETER INSTANCE = proc_sys_reset_0
 PARAMETER C_EXT_RESET_HIGH = 1
 PARAMETER HW_VER = 3.00.a
 PORT Slowest_sync_clk = sys_clk
 PORT Ext_Reset_In = sys_rst_s
 PORT MB_Debug_Sys_Rst = Debug_SYS_Rst
 PORT Dcm_locked = Dcm_all_locked
 PORT MB_Reset = mb_reset
 PORT Bus_Struct_Reset = sys_bus_reset
 PORT Peripheral_Reset = sys_periph_reset
END

BEGIN plb_led7seg
 PARAMETER INSTANCE = led7seg
 PARAMETER HW_VER = 1.00.a
 PARAMETER C_BASEADDR = 0x84C00000
 PARAMETER C_HIGHADDR = 0x84C0FFFF
 PARAMETER C_REFRESH_PERIOD_US = 4000
 PARAMETER C_SEGMENTS_ACTIVE_LOW = true
 PARAMETER C_ANODES_ACTIVE_LOW = true
 BUS_INTERFACE SPLB = mb_plb
 PORT segments = led7seg_segments
 PORT anodes = led7seg_anodes
 PORT switch_zeros = led7seg_switch_zeros
 PORT switch_off = led7seg_switch_off
END

BEGIN microblaze
 PARAMETER INSTANCE = microblaze_0
 PARAMETER C_AREA_OPTIMIZED = 1
 PARAMETER C_USE_BARREL = 1
 PARAMETER C_DEBUG_ENABLED = 1
 PARAMETER HW_VER = 8.10.a
 BUS_INTERFACE DLMB = dlmb
 BUS_INTERFACE ILMB = ilmb
 BUS_INTERFACE DPLB = mb_plb
 BUS_INTERFACE IPLB = mb_plb
 BUS_INTERFACE DEBUG = microblaze_0_mdm_bus
 PORT MB_RESET = mb_reset
 PORT INTERRUPT = int_control_0_Irq
END

BEGIN mdm
 PARAMETER INSTANCE = mdm_0
 PARAMETER C_MB_DBG_PORTS = 1
 PARAMETER C_USE_UART = 1
 PARAMETER HW_VER = 2.00.b
 PARAMETER C_BASEADDR = 0x84400000
 PARAMETER C_HIGHADDR = 0x8440ffff
 BUS_INTERFACE SPLB = mb_plb
 BUS_INTERFACE MBDEBUG_0 = microblaze_0_mdm_bus
 PORT Debug_SYS_Rst = Debug_SYS_Rst
END

BEGIN plb_v46
 PARAMETER INSTANCE = mb_plb
 PARAMETER HW_VER = 1.05.a
 PORT PLB_Clk = sys_clk
 PORT SYS_Rst = sys_bus_reset
END

BEGIN bram_block
 PARAMETER INSTANCE = lmb_bram
 PARAMETER HW_VER = 1.00.a
 BUS_INTERFACE PORTA = ilmb_port
 BUS_INTERFACE PORTB = dlmb_port
END

BEGIN xps_intc
 PARAMETER INSTANCE = int_control_0
 PARAMETER HW_VER = 2.01.a
 PARAMETER C_BASEADDR = 0x81800000
 PARAMETER C_HIGHADDR = 0x8180ffff
 BUS_INTERFACE SPLB = mb_plb
 PORT Intr = rs232_Interrupt
 PORT Irq = int_control_0_Irq
END

BEGIN lmb_bram_if_cntlr
 PARAMETER INSTANCE = ilmb_cntlr
 PARAMETER HW_VER = 3.00.a
 PARAMETER C_BASEADDR = 0x00000000
 PARAMETER C_HIGHADDR = 0x00003fff
 BUS_INTERFACE SLMB = ilmb
 BUS_INTERFACE BRAM_PORT = ilmb_port
END

BEGIN lmb_v10
 PARAMETER INSTANCE = ilmb
 PARAMETER HW_VER = 2.00.a
 PORT LMB_Clk = sys_clk
 PORT SYS_Rst = sys_bus_reset
END

BEGIN lmb_bram_if_cntlr
 PARAMETER INSTANCE = dlmb_cntlr
 PARAMETER HW_VER = 3.00.a
 PARAMETER C_BASEADDR = 0x00000000
 PARAMETER C_HIGHADDR = 0x00003fff
 BUS_INTERFACE SLMB = dlmb
 BUS_INTERFACE BRAM_PORT = dlmb_port
END

BEGIN lmb_v10
 PARAMETER INSTANCE = dlmb
 PARAMETER HW_VER = 2.00.a
 PORT LMB_Clk = sys_clk
 PORT SYS_Rst = sys_bus_reset
END

BEGIN clock_generator
 PARAMETER INSTANCE = clock_generator_0
 PARAMETER C_CLKIN_FREQ = 50000000
 PARAMETER C_CLKOUT0_FREQ = 50000000
 PARAMETER C_CLKOUT0_PHASE = 0
 PARAMETER C_CLKOUT0_GROUP = NONE
 PARAMETER C_CLKOUT0_BUF = TRUE
 PARAMETER C_EXT_RESET_HIGH = 1
 PARAMETER HW_VER = 4.01.a
 PORT CLKIN = CLK_S
 PORT CLKOUT0 = sys_clk
 PORT RST = sys_rst_s
 PORT LOCKED = Dcm_all_locked
END

