XPS Project Report

Printable Version

Overview

Resources Used
1 | MicroBlaze
1 | Processor Local Bus (PLB) 4.6
2 | Local Memory Bus (LMB) 1.0
1 | Block RAM (BRAM) Block
2 | LMB BRAM Controller
1 | XPS UART (Lite)
1 | Processor System Reset Module
1 | PLB_LED7SEG
1 | MicroBlaze Debug Module (MDM)
1 | XPS Interrupt Controller
1 | Clock Generator

Specifics
Generated | Tue Dec 13 14:27:19 2011
EDK Version | 13.1
Device Family | spartan3
Device | xc3s200ft256-4

Block Diagram | TOP
--- | ---

External Ports | TOP
--- | ---

These are the external ports defined in the MHS file.

Attributes Key
The attributes are obtained from the SIGIS and IOB_STATE parameters set on the PORT in the MHS file
CLK indicates Clock ports, (SIGIS = CLK)
INTR indicates Interrupt ports,(SIGIS = INTR)
RESET indicates Reset ports, (SIGIS = RST)
BUF or REG Indicates ports that instantiate or infer IOB primitives, (IOB_STATE = BUF or REG)

# | NAME | DIR | [LSB:MSB] | SIG | ATTRIBUTES
SHARED | fpga_0_rst_1_sys_rst_pin | I | 1 | sys_rst_s | RESET
clock_generator_0 | fpga_0_clk_1_sys_clk_pin | I | 1 | CLK_S | CLK
led7seg | fpga_0_led7seg_off_pin | I | 1 | led7seg_switch_off |
led7seg | fpga_0_led7seg_zeros_pin | I | 1 | led7seg_switch_zeros |
led7seg | fpga_0_led7seg_anodes_pin | O | 0:3 | led7seg_anodes |
led7seg | fpga_0_led7seg_segments_pin | O | 0:6 | led7seg_segments |
rs232 | fpga_0_RX_pin | I | 1 | rs232_RX |
rs232 | fpga_0_TX_pin | O | 1 | rs232_TX |
Unconnected | fpga_0_led7seg_dot_pin | O | 1 | net_vcc |

Processors | TOP
--- | ---

microblaze_0 MicroBlaze The MicroBlaze 32 bit soft processor

IP Specs
Core | Version | Documentation
--- | --- | ---
microblaze | 8.10.a | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | MB_RESET | I | 1 | mb_reset
1 | INTERRUPT | I | 1 | int_control_0_Irq
Bus Interfaces
NAME | TYPE | BUSSTD | BUS | Connected To
DLMB | MASTER | LMB | dlmb | dlmb_cntlr
ILMB | MASTER | LMB | ilmb | ilmb_cntlr
DPLB | MASTER | PLBV46 | mb_plb | 4 Peripherals.
IPLB | MASTER | PLBV46 | mb_plb | 4 Peripherals.
DEBUG | TARGET | XIL_MBDEBUG3 | microblaze_0_mdm_bus | mdm_0

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_SCO | 0
C_FREQ | 0
C_DATA_SIZE | 32
C_DYNAMIC_BUS_SIZING | 1
C_FAMILY | virtex5
C_INSTANCE | microblaze
C_FAULT_TOLERANT | 0
C_ECC_USE_CE_EXCEPTION | 0
C_ENDIANNESS | 0
C_AREA_OPTIMIZED | 1
C_OPTIMIZATION | 0
C_INTERCONNECT | 1
C_STREAM_INTERCONNECT | 0
C_DPLB_DWIDTH | 32
C_DPLB_NATIVE_DWIDTH | 32
C_DPLB_BURST_EN | 0
C_DPLB_P2P | 0
C_IPLB_DWIDTH | 32
C_IPLB_NATIVE_DWIDTH | 32
C_IPLB_BURST_EN | 0
C_IPLB_P2P | 0
C_M_AXI_DP_SUPPORTS_THREADS | 0
C_M_AXI_DP_THREAD_ID_WIDTH | 1
C_M_AXI_DP_SUPPORTS_READ | 1
C_M_AXI_DP_SUPPORTS_WRITE | 1
C_M_AXI_DP_SUPPORTS_NARROW_BURST | 0
C_M_AXI_DP_DATA_WIDTH | 32
C_M_AXI_DP_ADDR_WIDTH | 32
C_M_AXI_DP_PROTOCOL | AXI4LITE
C_M_AXI_DP_EXCLUSIVE_ACCESS | 0
C_INTERCONNECT_M_AXI_DP_READ_ISSUING | 1
C_INTERCONNECT_M_AXI_DP_WRITE_ISSUING | 1
C_M_AXI_IP_SUPPORTS_THREADS | 0
C_M_AXI_IP_THREAD_ID_WIDTH | 1
C_M_AXI_IP_SUPPORTS_READ | 1
C_M_AXI_IP_SUPPORTS_WRITE | 0
C_M_AXI_IP_SUPPORTS_NARROW_BURST | 0
C_M_AXI_IP_DATA_WIDTH | 32
C_M_AXI_IP_ADDR_WIDTH | 32
C_M_AXI_IP_PROTOCOL | AXI4LITE
C_INTERCONNECT_M_AXI_IP_READ_ISSUING | 1
C_D_AXI | 0
C_D_PLB | 0
C_D_LMB | 1
C_I_AXI | 0
C_I_PLB | 0
C_I_LMB | 1
C_USE_MSR_INSTR | 1
C_USE_PCMP_INSTR | 1
C_USE_BARREL | 1
C_USE_DIV | 0
C_USE_HW_MUL | 1
C_USE_FPU | 0
C_UNALIGNED_EXCEPTIONS | 0
C_ILL_OPCODE_EXCEPTION | 0
C_M_AXI_I_BUS_EXCEPTION | 0
C_M_AXI_D_BUS_EXCEPTION | 0
C_IPLB_BUS_EXCEPTION | 0
C_DPLB_BUS_EXCEPTION | 0
C_DIV_ZERO_EXCEPTION | 0
C_FPU_EXCEPTION | 0
C_FSL_EXCEPTION | 0
C_USE_STACK_PROTECTION | 0
C_PVR | 0
C_PVR_USER1 | 0x00
C_PVR_USER2 | 0x00000000
C_DEBUG_ENABLED | 1
C_NUMBER_OF_PC_BRK | 1
C_NUMBER_OF_RD_ADDR_BRK | 0
C_NUMBER_OF_WR_ADDR_BRK | 0
C_INTERRUPT_IS_EDGE | 0
C_EDGE_IS_POSITIVE | 1
C_RESET_MSR | 0x00000000
C_OPCODE_0x0_ILLEGAL | 0
C_FSL_LINKS | 0
C_FSL_DATA_SIZE | 32
C_USE_EXTENDED_FSL_INSTR | 0
C_M0_AXIS_PROTOCOL | GENERIC
C_S0_AXIS_PROTOCOL | GENERIC
C_M1_AXIS_PROTOCOL | GENERIC
C_S1_AXIS_PROTOCOL | GENERIC
C_M2_AXIS_PROTOCOL | GENERIC
C_S2_AXIS_PROTOCOL | GENERIC
C_M3_AXIS_PROTOCOL | GENERIC
C_S3_AXIS_PROTOCOL | GENERIC
C_M4_AXIS_PROTOCOL | GENERIC
C_S4_AXIS_PROTOCOL | GENERIC
C_M5_AXIS_PROTOCOL | GENERIC
C_S5_AXIS_PROTOCOL | GENERIC
C_M6_AXIS_PROTOCOL | GENERIC
C_S6_AXIS_PROTOCOL | GENERIC
C_M7_AXIS_PROTOCOL | GENERIC
C_S7_AXIS_PROTOCOL | GENERIC
C_M8_AXIS_PROTOCOL | GENERIC
C_S8_AXIS_PROTOCOL | GENERIC
C_M9_AXIS_PROTOCOL | GENERIC
C_S9_AXIS_PROTOCOL | GENERIC
C_M10_AXIS_PROTOCOL | GENERIC
C_S10_AXIS_PROTOCOL | GENERIC
C_M11_AXIS_PROTOCOL | GENERIC
C_S11_AXIS_PROTOCOL | GENERIC
C_M12_AXIS_PROTOCOL | GENERIC
C_S12_AXIS_PROTOCOL | GENERIC
C_M13_AXIS_PROTOCOL | GENERIC
C_S13_AXIS_PROTOCOL | GENERIC
C_M14_AXIS_PROTOCOL | GENERIC
C_S14_AXIS_PROTOCOL | GENERIC

Name | Value
C_M15_AXIS_PROTOCOL | GENERIC
C_S15_AXIS_PROTOCOL | GENERIC
C_M0_AXIS_DATA_WIDTH | 32
C_S0_AXIS_DATA_WIDTH | 32
C_M1_AXIS_DATA_WIDTH | 32
C_S1_AXIS_DATA_WIDTH | 32
C_M2_AXIS_DATA_WIDTH | 32
C_S2_AXIS_DATA_WIDTH | 32
C_M3_AXIS_DATA_WIDTH | 32
C_S3_AXIS_DATA_WIDTH | 32
C_M4_AXIS_DATA_WIDTH | 32
C_S4_AXIS_DATA_WIDTH | 32
C_M5_AXIS_DATA_WIDTH | 32
C_S5_AXIS_DATA_WIDTH | 32
C_M6_AXIS_DATA_WIDTH | 32
C_S6_AXIS_DATA_WIDTH | 32
C_M7_AXIS_DATA_WIDTH | 32
C_S7_AXIS_DATA_WIDTH | 32
C_M8_AXIS_DATA_WIDTH | 32
C_S8_AXIS_DATA_WIDTH | 32
C_M9_AXIS_DATA_WIDTH | 32
C_S9_AXIS_DATA_WIDTH | 32
C_M10_AXIS_DATA_WIDTH | 32
C_S10_AXIS_DATA_WIDTH | 32
C_M11_AXIS_DATA_WIDTH | 32
C_S11_AXIS_DATA_WIDTH | 32
C_M12_AXIS_DATA_WIDTH | 32
C_S12_AXIS_DATA_WIDTH | 32
C_M13_AXIS_DATA_WIDTH | 32
C_S13_AXIS_DATA_WIDTH | 32
C_M14_AXIS_DATA_WIDTH | 32
C_S14_AXIS_DATA_WIDTH | 32
C_M15_AXIS_DATA_WIDTH | 32
C_S15_AXIS_DATA_WIDTH | 32
C_ICACHE_BASEADDR | 0x00000000
C_ICACHE_HIGHADDR | 0x3FFFFFFF
C_USE_ICACHE | 0
C_ALLOW_ICACHE_WR | 1
C_ADDR_TAG_BITS | 17
C_CACHE_BYTE_SIZE | 8192
C_ICACHE_USE_FSL | 1
C_ICACHE_LINE_LEN | 4
C_ICACHE_ALWAYS_USED | 0
C_ICACHE_INTERFACE | 0
C_ICACHE_VICTIMS | 0
C_ICACHE_STREAMS | 0
C_ICACHE_FORCE_TAG_LUTRAM | 0
C_ICACHE_DATA_WIDTH | 0
C_M_AXI_IC_SUPPORTS_THREADS | 0
C_M_AXI_IC_THREAD_ID_WIDTH | 1
C_M_AXI_IC_SUPPORTS_READ | 1
C_M_AXI_IC_SUPPORTS_WRITE | 0
C_M_AXI_IC_SUPPORTS_NARROW_BURST | 0
C_M_AXI_IC_DATA_WIDTH | 32
C_M_AXI_IC_ADDR_WIDTH | 32
C_M_AXI_IC_PROTOCOL | AXI4
C_M_AXI_IC_USER_VALUE | 0b11111
C_M_AXI_IC_SUPPORTS_USER_SIGNALS | 1
C_M_AXI_IC_AWUSER_WIDTH | 5
C_M_AXI_IC_ARUSER_WIDTH | 5
C_M_AXI_IC_WUSER_WIDTH | 1
C_M_AXI_IC_RUSER_WIDTH | 1
C_M_AXI_IC_BUSER_WIDTH | 1
C_INTERCONNECT_M_AXI_IC_READ_ISSUING | 2
C_DCACHE_BASEADDR | 0x00000000
C_DCACHE_HIGHADDR | 0x3FFFFFFF
C_USE_DCACHE | 0
C_ALLOW_DCACHE_WR | 1
C_DCACHE_ADDR_TAG | 17
C_DCACHE_BYTE_SIZE | 8192
C_DCACHE_USE_FSL | 1
C_DCACHE_LINE_LEN | 4
C_DCACHE_ALWAYS_USED | 0
C_DCACHE_INTERFACE | 0
C_DCACHE_USE_WRITEBACK | 0
C_DCACHE_VICTIMS | 0
C_DCACHE_FORCE_TAG_LUTRAM | 0
C_DCACHE_DATA_WIDTH | 0
C_M_AXI_DC_SUPPORTS_THREADS | 0
C_M_AXI_DC_THREAD_ID_WIDTH | 1
C_M_AXI_DC_SUPPORTS_READ | 1
C_M_AXI_DC_SUPPORTS_WRITE | 1
C_M_AXI_DC_SUPPORTS_NARROW_BURST | 0
C_M_AXI_DC_DATA_WIDTH | 32
C_M_AXI_DC_ADDR_WIDTH | 32
C_M_AXI_DC_PROTOCOL | AXI4
C_M_AXI_DC_EXCLUSIVE_ACCESS | 0
C_M_AXI_DC_USER_VALUE | 0b11111
C_M_AXI_DC_SUPPORTS_USER_SIGNALS | 1
C_M_AXI_DC_AWUSER_WIDTH | 5
C_M_AXI_DC_ARUSER_WIDTH | 5
C_M_AXI_DC_WUSER_WIDTH | 1
C_M_AXI_DC_RUSER_WIDTH | 1
C_M_AXI_DC_BUSER_WIDTH | 1
C_INTERCONNECT_M_AXI_DC_READ_ISSUING | 2
C_INTERCONNECT_M_AXI_DC_WRITE_ISSUING | 32
C_USE_MMU | 0
C_MMU_DTLB_SIZE | 4
C_MMU_ITLB_SIZE | 2
C_MMU_TLB_ACCESS | 3
C_MMU_ZONES | 16
C_MMU_PRIVILEGED_INSTR | 0
C_USE_INTERRUPT | 0
C_USE_EXT_BRK | 0
C_USE_EXT_NM_BRK | 0
C_USE_BRANCH_TARGET_CACHE | 0
C_BRANCH_TARGET_CACHE_SIZE | 0

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

Debuggers | TOP
--- | ---

mdm_0 MicroBlaze Debug Module (MDM) Debug module for MicroBlaze Soft Processor.

IP Specs
Core | Version | Documentation
--- | --- | ---
mdm | 2.00.b | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | Debug_SYS_Rst | O | 1 | Debug_SYS_Rst
Bus Interfaces
NAME | TYPE | BUSSTD | BUS | Connected To
MBDEBUG_0 | INITIATOR | XIL_MBDEBUG3 | microblaze_0_mdm_bus | microblaze_0
SPLB | SLAVE | PLBV46 | mb_plb | 4 Peripherals.

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_FAMILY | virtex6
C_JTAG_CHAIN | 2
C_INTERCONNECT | 1
C_BASEADDR | 0x84400000
C_HIGHADDR | 0x8440FFFF
C_SPLB_AWIDTH | 32
C_SPLB_DWIDTH | 32
C_SPLB_P2P | 0
C_SPLB_MID_WIDTH | 3

Name | Value
C_SPLB_NUM_MASTERS | 8
C_SPLB_NATIVE_DWIDTH | 32
C_SPLB_SUPPORT_BURSTS | 0
C_MB_DBG_PORTS | 1
C_USE_UART | 1
C_S_AXI_ADDR_WIDTH | 32
C_S_AXI_DATA_WIDTH | 32
C_S_AXI_PROTOCOL | AXI4LITE

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

Interrupt Controllers | TOP
--- | ---

int_control_0 XPS Interrupt Controller intc core attached to the PLBV46

IP Specs
Core | Version | Documentation
--- | --- | ---
xps_intc | 2.01.a | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | Intr | I | 1 | rs232_Interrupt
1 | Irq | O | 1 | int_control_0_Irq
Bus Interfaces
NAME | TYPE | BUSSTD | BUS | Connected To
SPLB | SLAVE | PLBV46 | mb_plb | 4 Peripherals.
Interrupt Priorities
Priority | SIG | MODULE
0 | rs232_Interrupt | rs232

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_FAMILY | virtex5
C_BASEADDR | 0x81800000
C_HIGHADDR | 0x8180FFFF
C_SPLB_AWIDTH | 32
C_SPLB_DWIDTH | 32
C_SPLB_P2P | 0
C_SPLB_NUM_MASTERS | 1
C_SPLB_MID_WIDTH | 1
C_SPLB_NATIVE_DWIDTH | 32
C_SPLB_SUPPORT_BURSTS | 0

Name | Value
C_NUM_INTR_INPUTS | 2
C_KIND_OF_INTR | 0xFFFFFFFF
C_KIND_OF_EDGE | 0xFFFFFFFF
C_KIND_OF_LVL | 0xFFFFFFFF
C_HAS_IPR | 1
C_HAS_SIE | 1
C_HAS_CIE | 1
C_HAS_IVR | 1
C_IRQ_IS_LEVEL | 1
C_IRQ_ACTIVE | 1

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

Busses | TOP
--- | ---

dlmb Local Memory Bus (LMB) 1.0 'The LMB is a fast, local bus for connecting MicroBlaze I and D ports to peripherals and BRAM'

IP Specs
Core | Version | Documentation
--- | --- | ---
lmb_v10 | 2.00.a | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | LMB_Clk | I | 1 | sys_clk
1 | SYS_Rst | I | 1 | sys_bus_reset
Bus Connections
INSTANCE | INTERFACE TYPE | INTERFACE NAME
microblaze_0 | MASTER | DLMB
dlmb_cntlr | SLAVE | SLMB

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.
Name | Value
C_LMB_NUM_SLAVES | 4
C_LMB_AWIDTH | 32
C_LMB_DWIDTH | 32
C_EXT_RESET_HIGH | 1

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

ilmb Local Memory Bus (LMB) 1.0 'The LMB is a fast, local bus for connecting MicroBlaze I and D ports to peripherals and BRAM'

IP Specs
Core | Version | Documentation
--- | --- | ---
lmb_v10 | 2.00.a | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | LMB_Clk | I | 1 | sys_clk
1 | SYS_Rst | I | 1 | sys_bus_reset
Bus Connections
INSTANCE | INTERFACE TYPE | INTERFACE NAME
microblaze_0 | MASTER | ILMB
ilmb_cntlr | SLAVE | SLMB

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.
Name | Value
C_LMB_NUM_SLAVES | 4
C_LMB_AWIDTH | 32
C_LMB_DWIDTH | 32
C_EXT_RESET_HIGH | 1

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

mb_plb Processor Local Bus (PLB) 4.6 'Xilinx 64-bit Processor Local Bus (PLB) consists of a bus control unit, a watchdog timer, and separate address, write, and read data path units with a a three-cycle only arbitration feature'

IP Specs
Core | Version | Documentation
--- | --- | ---
plb_v46 | 1.05.a | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | PLB_Clk | I | 1 | sys_clk
1 | SYS_Rst | I | 1 | sys_bus_reset
Bus Connections
INSTANCE | INTERFACE TYPE | INTERFACE NAME
microblaze_0 | MASTER | DPLB
microblaze_0 | MASTER | IPLB
rs232 | SLAVE | SPLB
led7seg | SLAVE | SPLB
mdm_0 | SLAVE | SPLB
int_control_0 | SLAVE | SPLB

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_PLBV46_NUM_MASTERS | 4
C_PLBV46_NUM_SLAVES | 8
C_PLBV46_MID_WIDTH | 2
C_PLBV46_AWIDTH | 32
C_PLBV46_DWIDTH | 64
C_DCR_INTFCE | 0
C_BASEADDR | 0B1111111111
C_HIGHADDR | 0B0000000000
C_DCR_AWIDTH | 10

Name | Value
C_DCR_DWIDTH | 32
C_EXT_RESET_HIGH | 1
C_IRQ_ACTIVE | 1
C_NUM_CLK_PLB2OPB_REARB | 5
C_ADDR_PIPELINING_TYPE | 1
C_FAMILY | virtex5
C_P2P | 0
C_ARB_TYPE | 0

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

Memorys | TOP
--- | ---

lmb_bram Block RAM (BRAM) Block The BRAM Block is a configurable memory module that attaches to a variety of BRAM Interface Controllers.

IP Specs
Core | Version | Documentation
--- | --- | ---
bram_block | 1.00.a | IP

Bus Interfaces
NAME | TYPE | BUSSTD | BUS | Connected To
--- | --- | --- | --- | ---
PORTA | TARGET | XIL_BRAM | ilmb_port | ilmb_cntlr
PORTB | TARGET | XIL_BRAM | dlmb_port | dlmb_cntlr

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.
Name | Value
C_MEMSIZE | 2048
C_PORT_DWIDTH | 32
C_PORT_AWIDTH | 32
C_NUM_WE | 4
C_FAMILY | virtex2

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

Memory Controllers | TOP
--- | ---

dlmb_cntlr LMB BRAM Controller Local Memory Bus (LMB) Block RAM (BRAM) Interface Controller connects to an lmb bus

IP Specs
Core | Version | Documentation
--- | --- | ---
lmb_bram_if_cntlr | 3.00.a | IP

Bus Interfaces
NAME | TYPE | BUSSTD | BUS | Connected To
--- | --- | --- | --- | ---
BRAM_PORT | INITIATOR | XIL_BRAM | dlmb_port | lmb_bram
SLMB | SLAVE | LMB | dlmb | microblaze_0

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_BASEADDR | 0x00000000
C_HIGHADDR | 0x00003FFF
C_FAMILY | virtex5
C_MASK | 0x00800000
C_LMB_AWIDTH | 32
C_LMB_DWIDTH | 32
C_ECC | 0
C_INTERCONNECT | 0
C_FAULT_INJECT | 0
C_CE_FAILING_REGISTERS | 0
C_UE_FAILING_REGISTERS | 0
C_ECC_STATUS_REGISTERS | 0
C_ECC_ONOFF_REGISTER | 0
C_ECC_ONOFF_RESET_VALUE | 1
C_CE_COUNTER_WIDTH | 0
C_WRITE_ACCESS | 2

Name | Value
C_SPLB_CTRL_BASEADDR | 0xFFFFFFFF
C_SPLB_CTRL_HIGHADDR | 0x00000000
C_SPLB_CTRL_AWIDTH | 32
C_SPLB_CTRL_DWIDTH | 32
C_SPLB_CTRL_P2P | 0
C_SPLB_CTRL_MID_WIDTH | 1
C_SPLB_CTRL_NUM_MASTERS | 1
C_SPLB_CTRL_SUPPORT_BURSTS | 0
C_SPLB_CTRL_NATIVE_DWIDTH | 32
C_SPLB_CTRL_CLK_FREQ_HZ | 100000000
C_S_AXI_CTRL_ACLK_FREQ_HZ | 100000000
C_S_AXI_CTRL_BASEADDR | 0xFFFFFFFF
C_S_AXI_CTRL_HIGHADDR | 0x00000000
C_S_AXI_CTRL_ADDR_WIDTH | 32
C_S_AXI_CTRL_DATA_WIDTH | 32
C_S_AXI_CTRL_PROTOCOL | AXI4LITE

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

ilmb_cntlr LMB BRAM Controller Local Memory Bus (LMB) Block RAM (BRAM) Interface Controller connects to an lmb bus

IP Specs
Core | Version | Documentation
--- | --- | ---
lmb_bram_if_cntlr | 3.00.a | IP

Bus Interfaces
NAME | TYPE | BUSSTD | BUS | Connected To
--- | --- | --- | --- | ---
BRAM_PORT | INITIATOR | XIL_BRAM | ilmb_port | lmb_bram
SLMB | SLAVE | LMB | ilmb | microblaze_0

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_BASEADDR | 0x00000000
C_HIGHADDR | 0x00003FFF
C_FAMILY | virtex5
C_MASK | 0x00800000
C_LMB_AWIDTH | 32
C_LMB_DWIDTH | 32
C_ECC | 0
C_INTERCONNECT | 0
C_FAULT_INJECT | 0
C_CE_FAILING_REGISTERS | 0
C_UE_FAILING_REGISTERS | 0
C_ECC_STATUS_REGISTERS | 0
C_ECC_ONOFF_REGISTER | 0
C_ECC_ONOFF_RESET_VALUE | 1
C_CE_COUNTER_WIDTH | 0
C_WRITE_ACCESS | 2

Name | Value
C_SPLB_CTRL_BASEADDR | 0xFFFFFFFF
C_SPLB_CTRL_HIGHADDR | 0x00000000
C_SPLB_CTRL_AWIDTH | 32
C_SPLB_CTRL_DWIDTH | 32
C_SPLB_CTRL_P2P | 0
C_SPLB_CTRL_MID_WIDTH | 1
C_SPLB_CTRL_NUM_MASTERS | 1
C_SPLB_CTRL_SUPPORT_BURSTS | 0
C_SPLB_CTRL_NATIVE_DWIDTH | 32
C_SPLB_CTRL_CLK_FREQ_HZ | 100000000
C_S_AXI_CTRL_ACLK_FREQ_HZ | 100000000
C_S_AXI_CTRL_BASEADDR | 0xFFFFFFFF
C_S_AXI_CTRL_HIGHADDR | 0x00000000
C_S_AXI_CTRL_ADDR_WIDTH | 32
C_S_AXI_CTRL_DATA_WIDTH | 32
C_S_AXI_CTRL_PROTOCOL | AXI4LITE

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

Peripherals | TOP
--- | ---

led7seg PLB_LED7SEG PLB controller for the 7-segments led display

IP Specs
Core | Version
--- | ---
plb_led7seg | 1.00.a

PORT LIST
These are the ports listed in the MHS file.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | segments | O | 1 | led7seg_segments
1 | anodes | O | 1 | led7seg_anodes
2 | switch_zeros | I | 1 | led7seg_switch_zeros
3 | switch_off | I | 1 | led7seg_switch_off
Bus Interfaces
NAME | TYPE | BUSSTD | BUS | Connected To
SPLB | SLAVE | PLBV46 | mb_plb | 4 Peripherals.

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_BASEADDR | 0x84C00000
C_HIGHADDR | 0x84C0FFFF
C_SPLB_AWIDTH | 32
C_SPLB_DWIDTH | 128
C_SPLB_NUM_MASTERS | 8
C_SPLB_MID_WIDTH | 3
C_SPLB_NATIVE_DWIDTH | 32
C_SPLB_P2P | 0

Name | Value
C_SPLB_SUPPORT_BURSTS | 0
C_SPLB_SMALLEST_MASTER | 32
C_SPLB_CLK_PERIOD_PS | 10000
C_INCLUDE_DPHASE_TIMER | 0
C_FAMILY | virtex6
C_REFRESH_PERIOD_US | 4000
C_SEGMENTS_ACTIVE_LOW | true
C_ANODES_ACTIVE_LOW | true

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

rs232 XPS UART (Lite) Generic UART (Universal Asynchronous Receiver/Transmitter) for PLBV46 bus.

IP Specs
Core | Version | Documentation
--- | --- | ---
xps_uartlite | 1.01.a | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | RX | I | 1 | rs232_RX
1 | TX | O | 1 | rs232_TX
2 | Interrupt | O | 1 | rs232_Interrupt
Bus Interfaces
NAME | TYPE | BUSSTD | BUS | Connected To
SPLB | SLAVE | PLBV46 | mb_plb | 4 Peripherals.

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_FAMILY | virtex5
C_SPLB_CLK_FREQ_HZ | 100000000
C_BASEADDR | 0x84000000
C_HIGHADDR | 0x8400FFFF
C_SPLB_AWIDTH | 32
C_SPLB_DWIDTH | 32
C_SPLB_P2P | 0
C_SPLB_MID_WIDTH | 1

Name | Value
C_SPLB_NUM_MASTERS | 1
C_SPLB_SUPPORT_BURSTS | 0
C_SPLB_NATIVE_DWIDTH | 32
C_BAUDRATE | 115200
C_DATA_BITS | 8
C_USE_PARITY | 0
C_ODD_PARITY | 1

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

IP | TOP
--- | ---

clock_generator_0 Clock Generator Clock generator for processor system.

IP Specs
Core | Version | Documentation
--- | --- | ---
clock_generator | 4.01.a | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | CLKIN | I | 1 | CLK_S
1 | CLKOUT0 | O | 1 | sys_clk
2 | RST | I | 1 | sys_rst_s
3 | LOCKED | O | 1 | Dcm_all_locked

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.

Name | Value
C_FAMILY | virtex6
C_DEVICE | NOT_SET
C_PACKAGE | NOT_SET
C_SPEEDGRADE | NOT_SET
C_CLKIN_FREQ | 50000000
C_CLKOUT0_FREQ | 50000000
C_CLKOUT0_PHASE | 0
C_CLKOUT0_GROUP | NONE
C_CLKOUT0_BUF | TRUE
C_CLKOUT0_VARIABLE_PHASE | FALSE
C_CLKOUT1_FREQ | 0
C_CLKOUT1_PHASE | 0
C_CLKOUT1_GROUP | NONE
C_CLKOUT1_BUF | TRUE
C_CLKOUT1_VARIABLE_PHASE | FALSE
C_CLKOUT2_FREQ | 0
C_CLKOUT2_PHASE | 0
C_CLKOUT2_GROUP | NONE
C_CLKOUT2_BUF | TRUE
C_CLKOUT2_VARIABLE_PHASE | FALSE
C_CLKOUT3_FREQ | 0
C_CLKOUT3_PHASE | 0
C_CLKOUT3_GROUP | NONE
C_CLKOUT3_BUF | TRUE
C_CLKOUT3_VARIABLE_PHASE | FALSE
C_CLKOUT4_FREQ | 0
C_CLKOUT4_PHASE | 0
C_CLKOUT4_GROUP | NONE
C_CLKOUT4_BUF | TRUE
C_CLKOUT4_VARIABLE_PHASE | FALSE
C_CLKOUT5_FREQ | 0
C_CLKOUT5_PHASE | 0
C_CLKOUT5_GROUP | NONE
C_CLKOUT5_BUF | TRUE
C_CLKOUT5_VARIABLE_PHASE | FALSE
C_CLKOUT6_FREQ | 0
C_CLKOUT6_PHASE | 0
C_CLKOUT6_GROUP | NONE
C_CLKOUT6_BUF | TRUE
C_CLKOUT6_VARIABLE_PHASE | FALSE
C_CLKOUT7_FREQ | 0
C_CLKOUT7_PHASE | 0
C_CLKOUT7_GROUP | NONE
C_CLKOUT7_BUF | TRUE
C_CLKOUT7_VARIABLE_PHASE | FALSE
C_CLKOUT8_FREQ | 0
C_CLKOUT8_PHASE | 0
C_CLKOUT8_GROUP | NONE

Name | Value
C_CLKOUT8_BUF | TRUE
C_CLKOUT8_VARIABLE_PHASE | FALSE
C_CLKOUT9_FREQ | 0
C_CLKOUT9_PHASE | 0
C_CLKOUT9_GROUP | NONE
C_CLKOUT9_BUF | TRUE
C_CLKOUT9_VARIABLE_PHASE | FALSE
C_CLKOUT10_FREQ | 0
C_CLKOUT10_PHASE | 0
C_CLKOUT10_GROUP | NONE
C_CLKOUT10_BUF | TRUE
C_CLKOUT10_VARIABLE_PHASE | FALSE
C_CLKOUT11_FREQ | 0
C_CLKOUT11_PHASE | 0
C_CLKOUT11_GROUP | NONE
C_CLKOUT11_BUF | TRUE
C_CLKOUT11_VARIABLE_PHASE | FALSE
C_CLKOUT12_FREQ | 0
C_CLKOUT12_PHASE | 0
C_CLKOUT12_GROUP | NONE
C_CLKOUT12_BUF | TRUE
C_CLKOUT12_VARIABLE_PHASE | FALSE
C_CLKOUT13_FREQ | 0
C_CLKOUT13_PHASE | 0
C_CLKOUT13_GROUP | NONE
C_CLKOUT13_BUF | TRUE
C_CLKOUT13_VARIABLE_PHASE | FALSE
C_CLKOUT14_FREQ | 0
C_CLKOUT14_PHASE | 0
C_CLKOUT14_GROUP | NONE
C_CLKOUT14_BUF | TRUE
C_CLKOUT14_VARIABLE_PHASE | FALSE
C_CLKOUT15_FREQ | 0
C_CLKOUT15_PHASE | 0
C_CLKOUT15_GROUP | NONE
C_CLKOUT15_BUF | TRUE
C_CLKOUT15_VARIABLE_PHASE | FALSE
C_CLKFBIN_FREQ | 0
C_CLKFBIN_DESKEW | NONE
C_CLKFBOUT_FREQ | 0
C_CLKFBOUT_PHASE | 0
C_CLKFBOUT_GROUP | NONE
C_CLKFBOUT_BUF | TRUE
C_PSDONE_GROUP | NONE
C_EXT_RESET_HIGH | 1
C_CLK_PRIMITIVE_FEEDBACK_BUF | FALSE
C_CLK_GEN | UPDATE

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

proc_sys_reset_0 Processor System Reset Module Reset management module

IP Specs
Core | Version | Documentation
--- | --- | ---
proc_sys_reset | 3.00.a | IP

PORT LIST
These are the ports listed in the MHS file. Please refer to the IP documentation for complete information about module ports.
# | NAME | DIR | [LSB:MSB] | SIGNAL
--- | --- | --- | --- | ---
0 | Slowest_sync_clk | I | 1 | sys_clk
1 | Ext_Reset_In | I | 1 | sys_rst_s
2 | MB_Debug_Sys_Rst | I | 1 | Debug_SYS_Rst
3 | Dcm_locked | I | 1 | Dcm_all_locked
4 | MB_Reset | O | 1 | mb_reset
5 | Bus_Struct_Reset | O | 1 | sys_bus_reset
6 | Peripheral_Reset | O | 1 | sys_periph_reset

Parameters
These are the current parameter settings for this module. Parameters marked with yellow indicate parameters set by the user. Parameters marked with blue indicate parameters set by the system.
Name | Value
C_SUBFAMILY | lx
C_EXT_RST_WIDTH | 4
C_AUX_RST_WIDTH | 4
C_EXT_RESET_HIGH | 1
C_AUX_RESET_HIGH | 1
C_NUM_BUS_RST | 1
C_NUM_PERP_RST | 1
C_NUM_INTERCONNECT_ARESETN | 1
C_NUM_PERP_ARESETN | 1
C_FAMILY | virtex5

Post Synthesis Device Utilization
Device utilization information is not available for this IP. Run platgen to generate synthesis information.

Timing Information | TOP
--- | ---

Post Synthesis Clock Limits
No clocks could be identified in the design. Run platgen to generate synthesis information.